Scotts Valley Community Performing Arts Center

Updated 6/8/2023

Facility Information 

Location: 251B Kings Village Road, Scotts Valley CA, 95066
Left end of the building that is shared with the Scotts Valley Library.

Management: Scotts Valley Community Theater Guild
A 501c3 Non-Profit organization, Federal Tax ID Number:  46-2791127
A 501c3 Non-Prot organization
Federal Tax ID Number:  46-2791127
Website: www.svctheaterguild.com
Mail to: P. O. Box 66438, Scotts Valley, CA 95067-6438

Contacts: 
Theater Operations Director – Ray Gorski – 831-252-3501, rgorski28@sbcglobal.net
Facilities Director – Mike Smith – 831-566-6576, mijarvis@aol.com
Technical Director - Lee Besse – 831-345-3426, Lee@besseworld.com
President, SVCTG: Larry Smith - 415-290-6307, larrysmith7@gmail.com

Overview

1. The Scotts Valley Performing Arts Center is a configurable facility measuring 96’ x 96’ with an 18’ high ceiling.

2. Entry and Exit
a. 2 double doors at front of building
b. 1 double door + 1 single door at rear of building
c. 1 roll up door (8’wx10’h) at rear of building, stage left
d. Lobby: 57’ x 20’ x 10’h (to lights).

3. The performance area:
a. Currently arranged in Proscenium configuration.  
b. The stage (4’x8’ modules) and seat modules (11 seats each) can be reconfigured (with some difficulty) to add, remove or rearrange stage and/or seats.
c. There is no orchestra pit.  A small orchestra can be located in the wings on stage right.

4. There is a 20’w x 11’h retractable projection screen mounted above down center stage behind the stage curtain and the first valence.

5. Restrooms are external in the rear of the building – 4 Mens + 4 Womens + 1 ADA.
6. Dressing and Green Rooms are available inside but it are not sound proof.  


Facility Specifications

1. Overall Proscenium Stage, Audience and Curtain layout
a. (See Attached diagram)

2. Proscenium configuration:
a. Seating Capacity - 264 theater seats (11 fixed per platform).
b. Designated area for 10 ADA + 10 companions in front.
c. Audience envelope is enclosed with curtains.

3. Stage Dimensions: 
a. Performance Area: 40’ x 28’.
b. Wings: ~24’ Stage Left and ~24’ Stage Right.

4. Curtains:
a. Full Retractable Down Stage Curtain - operates from Stage Left
b. Full Retractable Mid Stage Curtain - operates from Stage Right
c. Front Curtain line to rear wall – 24’
d. Optional Dead Hung Curtain upstage (reduces performance depth by ~4’)
e. Rear Cyc: 29’w x 11’h (to Valance)
f. Legs: 3 each - stage right and stage left

5. Heights:
a. Stage deck above floor: 39”
b. Stage height from deck to pipes: 14’
c. Stage height to from deck to Valance – 11’
d. House height to Glue Lam beams – 18’.
e. House height to roof - 21’.

6. Stairs to stage on stage right and stage left (outside audience envelope).
7. ADA lift to stage on stage left (outside audience envelope).

8. Stage loading:
9. Primary loading access through front doors.
10. Alternate Roll up door in rear at corner of building at Stage Left - 8’w x 10’h.
11. Fork Lift & Genie Scissor lifts available (require prior approval to operate).
12. 



Electrical Specifications


Lighting
1. Control Deck is not ADA accessible
2. Control System: 
a. ETC9648 – DMX Programmable
b. 96 Channels / sliders +96 Programmable
c. 24 Submasters
d. 180 Dimmers
3. Follow Spots: 2 - Satellite 1
a. 575 Watts HMI


Sound
1. Control deck is not ADA accessible
2. Mixer: Mackie Mixing Console 32.8.2 8-Bus
3. Amp: QSC, PLX1104 Power Amp for 4 main speakers on and above stage.
4. Amp: QSC, PLX3602 Power Amp for 2 Subwoofer Speakers under stage
5. Connection to recorder sound on sound deck:
a. 1/8” plug 
b. Blue Tooth
6. Speakers: 
a. 2 On Stage Speakers 
b. 2 Above Stage Speakers - EAW MK2366
c. 2 Subwoofer Speakers below stage
7. Microphones: Microphones, stands and cable are available at added cost.

a. 4 – Shure SM58
b. 2 – Shure BG5.1
c. 1 – Shure BG4.1
d. 2 – Shure 57
e. 2 – Sennheiser 835
f. 3 - Shure Beta 58.A

8. Mic Stands:
a. 13 – 3 leg
b. 8 – Single Pole
9. On Stage Electrics:
a. 2 Snakes – 75’ in Stage Left Wing. 1 up stage + 1 down stage.
10. Intercom Communication:
a. 6 – Hollyview Solidcom wireless headsets
11. No Hearing assist



Video
Control room is not ADA accessible

Projection:
· 1 On deck
· 1 mounted above stage for the Cyc 
· 3 Projectors in house are not currently functional.


Theater equipment not included in rent.  
(Quoted separately)

1. Baby Grand Piano
2. Wired and Wireless Microphones
3. Spotlights
4. Additional lighting for specials


